**Forced Induction Interchillers Order Form**

Name:

Street Address:

Suburb/City:

State:

Post Code:

Country:

Contact Phone Number:

Shipping address if different:

**Have read and understood terms and conditions:** YES/NO

**Chiller Information:**

Chiller Type: Race chiller

Competition Solenoid: YES/NO

Stage 2 Upgrade: YES/NO

T-Shirt Size: M, L, XL, 2XL

**Reservoir and Intercooler Pump Options:**

12L Holden/HSV---VE/VF Reservoir: YES/NO

Foam Insulation for 12L Reservoir: YES/NO

1.7gal Pontiac G8/Chevy SS---VE/VF Reservoir: YES/NO

Half Spare wheel reservoir tank: YES/NO

Reprogrammed Stewart EMP Intercooler pump: YES/NO

-16AN Fittings added to the EMP intercooler pump: YES/NO

**Blower Spacer Plate Options:**

LS3/L98/L77/LSA/LS9 Blower Spacer Plates: YES/NO

LS1/LS2 Blower Spacer Plates: YES/NO

LSA Blower Lid spacer: YES/NO

Thermal Reduction Blanket: YES/NO
Hellcat, Trackhawk, Demon blower spacer plates + thermal blanket: YES/NO

**Water fittings:**

AN-12 Pushlock water fittings: YES/NO

LSA Braided hose kit AN-16/12: YES/NO

**Car Details:**

Customer Name:

Make/Model/Year:

Supercharger/Turbocharger:

**What is not supplied with the interchiller kit:**

1. We do not supply electrical wiring, 15amp inline fuse or a relay this should be supplied and installed by a qualified auto electrician for the competition solenoid. We do not wish to be held accountable for dodgy wiring so we don’t supply it.

2. AN-12 fittings for the chiller these can either be push on style or traditional screw on style, this is a personal choice so we leave it up to you. (Unless you order it above in the options)

3. Intercooler hose is not supplied we recommend braided hose it looks neat and will not condensate, rubber hose can be used but will need to be foam sleeved to stop condensation forming. Braid also keeps cold in and heat out.

Everything else is supplied in the kit that you will require.

**Terms and conditions:**

No work will begin to take place on building your system until such time as payment has been received.

Any lead times provided to you are estimated lead times, we will do our best to be within that estimated time frame.

Forced Induction Interchillers does not make any guarantees that our interchiller system or associated components/products will be able to achieve any particular horsepower gain, intake or cabin temperatures that may have been seen in our images/videos, other workshop images/videos or customer images/videos. There are many variables that effect results, such as car make/model/year supercharger or turbocharger make/model/year, ambient weather conditions, installation/tuning and refrigerant charge.

Forced Induction Interchillers are not liable for any unforeseen labour during the installation of our products that you may incur.

Forced Induction Interchillers are not liable for any broken or damaged components on your vehicle such as but not limited to parts associated to the AC system, intercooler system, engine, chassis, drive line.

Forced Induction Interchillers warranties our parts provided for a period of 12 months, if a component is deemed to have failed it will be replaced free of charge, including shipment to you. Should you decide to pick up a replacement component from a supplier we are not liable for any travel expenses and we are also not liable to purchase the component for you if the component is not supplied directly from Forced Induction Interchillers, unless we have made prior payment arrangements with a distributor or directly with you the customer.

You the customer understand by filling out this order form selecting yes to having read the terms and conditions set out in this document that you are in agreement with these terms and conditions of this document.

**If possible email this form back to us in word doc format, our email address is:** info@fiinterchillers.com